**Pilot:** RED CAP five one niner seven ready lineup.

**ATC:** RED CAP five one niner seven runway two six , clear for takeoff

**Pilot:** Clear for takeoff runway two six RED CAP five one niner seven

**Pilot:** RED CAP five one niner seven passing two thousand, request heading two four five due weather.

**ATC:** Copy, RED CAP five one niner seven fly heading two four five

**Pilot:** RED CAP five one niner seven

**ATC:** RED CAP five one niner seven climb flight level one eight zero

**Pilot:** Climb flight level one niner zero, RED CAP five one niner seven

**ATC:** Negative, Climb flight level one eight zero

**Pilot:** flight level one eight zero, RED CAP five one niner seven

**ATC:** and report passing flight level one four zero thank you

**Pilot:** Report passing flight level one four zero, RED CAP five one niner seven

**Pilot:** RED CAP five one niner seven passing flight level one four zero

**ATC:** RED CAP five one niner seven continue climb flight level one eight zero and maintain heading, switch to one six zero decimal six

**Pilot:** Maintain heading, continue climb flight level one eight zero, switching to one six zero decimal six RED CAP five one niner seven

**ATC:** SINGAPORE three eight four two heavy turn right heading zero one zero, maintain three thousand feet

**Pilot:** heavy turn zero one zero, maintain three thousand, SINGAPORE three eight four two.

**Pilot:** Singapore Tower, GO CAT four two niner

**ATC:** GO CAT four two niner, Singapore Tower, go ahead

**Pilot:** GO CAT four two niner, request ATC clearance to Kuala Lumpur, flight level two three zero

**ATC:** GO CAT four two niner , cleared to Kuala Lumpur, via flight planned route, flight level two three zero, squawk two four zero zero

**Pilot:** GO CAT four two niner, cleared to Kuala Lumpur, via flight planned route, flight level two three zero, squawk two four zero zero

**ATC:** GO CAT four two niner, contact Singapore Ground one two zero decimal three

**Pilot:** contact Singapore Ground one two zero decimal three, GO CAT four two niner

**Pilot:** Singapore Tower, JETSTAR eight seven three, ready for departure

**ATC:** JETSTAR eight seven three, surface wind two zero zero degrees, one zero knots, climb to three thousand feet, runway two six, cleared for takeoff

**Pilot:**  cleared to takeoff runway two six, climb three thousand feet. JETSTAR eight seven three

**ATC:** JETSTAR eight seven three, climb flight level one six zero, report passing flight level one two zero

**Pilot:** climb flight level one six zero, report passing flight level one two zero, JETSTAR eight seven three

**Pilot:** Singapore Tower,SINGAPORE three eight four two, finals, runway two six.

**ATC:** SINGAPORE three eight four two, clear to land, runway two six wind two seven zero degrees, one zero knots

**Pilot:** Cleared to land runway two six, SINGAPORE three eight four two

**Pilot:** JETSTAR eight seven three passing flight level one two zero

**ATC:** JETSTAR eight seven three, contact Singapore departure one two four decimal six

**Pilot:** Contact Singapore Departure, one two four decimal six JETSTAR eight seven three

**Pilot:** Singapore Tower, GO CAT four two niner, lined up runway two six, ready for departure

**ATC:** GO CAT four two niner, Singapore Tower, surface wind two two zero degrees, eight knots, climb to three thousand feet, runway two six, cleared for takeoff

**Pilot:** clear takeoff runway two six, climb three thousand, GO CAT four two niner

**Pilot:** Singapore Tower,SKYBIRD six zero two, currently holding over PAPA

**ATC:** SKYBIRD six zero two, Singapore Tower, go ahead

**Pilot:** Requesting to land due to bingo fuel, SKYBIRD six zero two

**ATC:** Copy, SKYBIRD six zero two turn left heading zero niner zero descent niner thousand feet

**Pilot:** left turn heading zero niner zero, descent niner thousand feet, SKYBIRD six zero two

**ATC:** GO CAT four two niner, climb flight level one niner zero, report passing flight level one four zero

**Pilot:** climb flight level one niner zero, report passing flight level one four zero, GO CAT four two niner

**ATC:** SKYBIRD six zero two, report finals

**Pilot:** SKYBIRD six zero two, finals, runway two six

**ATC:** SKYBIRD six zero two, clear to land, runway two six wind two three zero degrees, one two knots

**Pilot:** Cleared to land runway two six, SKYBIRD six zero two

**Pilot:** GO CAT four two niner, passing flight level one four zero at this time

**ATC:** GO CAT four two niner contact Singapore departure one two four decimal six

**Piot:** one two four decimal six, GO CAT four two niner. Good day